# Software Information
display_name = "Sega - Saturn (Emir)"
authors = "StrikerX3"
supported_extensions = "cue|chd|mds|ccd|iso|m3u"
corename = "Emir"
categories = "Emulator"
license = "GPLv3"
permissions = ""
display_version = "v0.3.3"

# Hardware Information
manufacturer = "Sega"
systemname = "Saturn"
systemid = "sega_saturn"
database = "Sega - Saturn"

# Libretro Features
supports_no_game = "false"
hw_render = "false"
needs_fullpath = "true"
disk_control = "true"
savestate = "true"
savestate_features = "deterministic"
cheats = "true"
input_descriptors = "true"
memory_descriptors = "true"
libretro_saves = "true"
core_options = "true"
load_subsystem = "false"
is_experimental = "true"

# Firmware / BIOS
firmware_count = 3
firmware0_desc = "sega_101.bin (Saturn JP BIOS)"
firmware0_path = "sega_101.bin"
firmware0_opt = "true"
firmware1_desc = "mpr-17933.bin (Saturn US/EU BIOS)"
firmware1_path = "mpr-17933.bin"
firmware1_opt = "true"
firmware2_desc = "saturn_bios.bin (Saturn BIOS)"
firmware2_path = "saturn_bios.bin"
firmware2_opt = "true"
notes = "(!) Requires a Saturn BIOS in the system directory.|(!) Any one of the three supported BIOS files will work: sega_101.bin, mpr-17933.bin, or saturn_bios.bin|(!) sega_101.bin (md5): 85ec9ca47d8f6807718151cbcca8b964|(!) mpr-17933.bin (md5): 3240872c70984b6cbfda1586cab68dbe|(!) Optional: CD Block LLE requires a 64KB CD block ROM placed in the system/cdb/ directory."

description = "A port of the Ymir Sega Saturn emulator to libretro. Ymir is a work-in-progress Saturn emulator focused on accuracy and compatibility. It features software rendering, SH2 emulation with optional cache emulation, and a modern codebase. A young but rapidly maturing alternative to Beetle Saturn."
